|  |  |  |  |
| --- | --- | --- | --- |
|  | |  | | --- | | **Simulation of Adapter Plate - 2017**  **Date: 03 October 2017 Designer: Solidworks**  **Study name: SimulationXpress Study**  **Analysis type: Static** | | Table of Contents  [Description 1](#_Toc494828892)  [Assumptions 2](#_Toc494828893)  [Model Information 2](#_Toc494828894)  [Material Properties 3](#_Toc494828895)  [Loads and Fixtures 3](#_Toc494828896)  [Mesh information 4](#_Toc494828897)  [Study Results 6](#_Toc494828898)  [Conclusion 8](#_Toc494828899) | |
| Description No Data |

|  |
| --- |
| Assumptions |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Model Information  |  |  |  |  |  | | --- | --- | --- | --- | --- | | |  | | --- | |  |   ****Model name:** Adapter Plate - 2017**  ****Current Configuration:** Default** | | | | | ****Solid Bodies**** | | | | | ****Document Name and Reference**** | ****Treated As**** | ****Volumetric Properties**** | ****Document Path/Date Modified**** | | **Boss-Extrude1** | **Solid Body** | ****Mass:0.18173 kg****  ****Volume:6.73072e-005 m^3****  ****Density:2700 kg/m^3****  ****Weight:1.78095 N**** | ****C:\Users\dunca\Documents\Uni\LunarSolidworks\Leg Adapter Plate\Adapter Plate - 2017.SLDPRT****  **Oct 03 20:32:15 2017** | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Material Properties  |  |  |  | | --- | --- | --- | | ****Model Reference**** | ****Properties**** | ****Components**** | |  | |  |  | | --- | --- | | ****Name:**** | **1060 Alloy** | | ****Model type:**** | **Linear Elastic Isotropic** | | ****Default failure criterion:**** | **Unknown** | | ****Yield strength:**** | **27.5742 N/mm^2** | | ****Tensile strength:**** | **68.9356 N/mm^2** | | **SolidBody 1(Boss-Extrude1)(Adapter Plate - 2017)** | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Loads and Fixtures**  | ****Fixture name**** | ****Fixture Image**** | ****Fixture Details**** | | --- | --- | --- | | **Fixed-1** |  | |  |  | | --- | --- | | Entities: | **6 face(s)** | | Type: | **Fixed Geometry** | |  | ****Load name**** | ****Load Image**** | ****Load Details**** | | --- | --- | --- | | **Force-1** |  | |  |  | | --- | --- | | Entities: | **10 face(s), 1 plane(s)** | | Reference: | **Front Plane** | | Type: | **Apply force** | | Values: | **---, ---, 274.68 N** | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Mesh information  |  |  | | --- | --- | | Mesh type | Solid Mesh | | Mesher Used: | Standard mesh | | Automatic Transition: | Off | | Include Mesh Auto Loops: | Off | | Jacobian points | 4 Points | | Element Size | 4.06905 mm | | Tolerance | 0.203452 mm | | Mesh Quality | High |  Mesh information - Details  |  |  | | --- | --- | | Total Nodes | 15335 | | Total Elements | 8524 | | Maximum Aspect Ratio | 4.2414 | | % of elements with Aspect Ratio < 3 | 99.4 | | % of elements with Aspect Ratio > 10 | 0 | | % of distorted elements(Jacobian) | 0 | | Time to complete mesh(hh;mm;ss): | 00:00:01 | | Computer name: | DRH-PC | |  | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Study Results  | Name | Type | Min | Max | | --- | --- | --- | --- | | Stress | VON: von Mises Stress | 0.0106883 N/mm^2 (MPa)  Node: 12443 | 6.23094 N/mm^2 (MPa)  Node: 15112 | | **Adapter Plate - 2017-SimulationXpress Study-Stress-Stress** | | | |  | Name | Type | Min | Max | | --- | --- | --- | --- | | Displacement | URES: Resultant Displacement | 0 mm  Node: 1 | 0.00475237 mm  Node: 12443 | | **Adapter Plate - 2017-SimulationXpress Study-Displacement-Displacement** | | | |  | Name | Type | | --- | --- | | Deformation | Deformed shape | | **Adapter Plate - 2017-SimulationXpress Study-Displacement-Deformation** | |  | Name | Type | Min | Max | | --- | --- | --- | --- | | Factor of Safety | Max von Mises Stress | 4.42537  Node: 15112 | 2579.85  Node: 12443 | | **Adapter Plate - 2017-SimulationXpress Study-Factor of Safety-Factor of Safety** | | | | |

|  |
| --- |
| Conclusion |